How to update SD4 aircraft firmware:

1. Unzip the “SwellproFirmwareTool”, and then run the “SharkFirmwareV2.exe”, choose the firmware in bar “2”. And make sure bar “2” is chosen (blue dot).

When the aircraft is shut down, connect the drone and computer with a USB cable. Power on the drone, and click the "update" button to start the update. When the progress reaches 100, it means that the upgrade has been successful!

After updating, restart the drone

图形用户界面, 文本, 应用程序

描述已自动生成

1. "SwellproFirmwareTool"의 압축을 풀고 "SharkFirmwareV2.exe"를 실행하고 "2" 막대에서 펌웨어를 선택합니다. 그리고 막대 "2"가 선택되었는지 확인합니다(파란색 점).

기체가 꺼지면 USB 케이블로 드론과 컴퓨터를 연결합니다. 드론의 전원을 켜고 "업데이트" 버튼을 클릭하여 업데이트를 시작합니다. 진행 상황이 100에 도달하면 업그레이드가 성공한 것입니다!

업데이트 후 드론 재시작