How to update SD4 remote control firmware:

1. Unzip the “SwellproFirmwareTool”, and then run the “SharkFirmwareV2.exe”, choose the firmware in bar “0”, and make sure bar “0” is chosen (blue dot).

2. Power on the remote controller, connect it to PC with a micro-USB cable. You can ignore any Windows messages about the USB device. Keep pressing the Power Button, then click the “Update” button in the Shart Firmware Tool, and wait for the progress indicator to reach 100% and go bright. Then release the remote controller power button - the update is done.

After upgrading, you need to restart the remote controller.

